**OLIVER TRAILER CHECKLIST**

Rev 02/18/18

|  |  |  |  |
| --- | --- | --- | --- |
| **ITEM** | **TOWING** | **CAMPING** | **COMMENT** |
| Exterior lights | OFF/ Check operation | As needed | Check running and brake lights each time plugged into truck. |
| Tires and wheels | Pressure and condition | Chocked | Check tires/ hubs temperature manually at stops. Visually inspect lug nuts and tread. 80 psi recommended. |
| Solar panels | Inspect |  | Walk around: visually inspect wire ties on knobs for security. |
| Exterior door, hatches, ports | Closed/ locked | As needed | Ensure battery tray is latched closed. |
| Steps | Raised | Lowered |  |
| Bulldog coupler | Latched/ locked | Latched/ locked | Never leave unlocked. Lube each trip. |
| Tongue jack | Raised | Lowered | On block |
| Rear stabilizers | Raised | As needed | On blocks |
| Chocks, blocks, pads | Stowed | Tires/ stabilizers | Rear compartment, doghouse |
| Safety cables, breakaway switch | Connected | Disconnected | Check BAS operation before first tow of trip |
| Trailer cable | Connected | Disconnected |  |
| 120V cord, 30A or 15A | Stowed | As needed | Rear compartment |
| Fresh water hose, regulator, filter | Stowed | As needed | Rear compartment, cap all open ports |
| Waste water hoses | Stowed | As needed | Rear bumper, ensure dump valves and 3 inch cover secured. |
| Water heater, water pump | OFF | ON | Turn ON WH switch (outside under cover) if on 120 V AC power |
| Bathroom Shutoff Valve | CLOSED | OPEN |  |
| Propane tanks | ON | ON | Keep unused bottle OFF to prevent running out of fuel, service in-use bottle when empty |
| Refrigerator | ON/ Propane | On/ Propane | Auto-switches to 120 V AC, do not run on DC when stationary. Must be close to level for proper operation. |
| Microwave oven glass tray | Stowed | In oven | Place glass tray and pinwheel in sink on a towel. |
| Awning/ handle/ brace/ tie downs | Stowed | As needed | Check 2 red security latches, flush when closed. Do not use in windy conditions. |
| Drawers/ pantry and bathroom doors | Secured |  | Latch 3 doors, secure all loose objects |
| Windows/ Blinds | Closed/Lowered |  | Bathroom window OK to leave open |
| Bathroom vent | Closed | Open | Fan OFF when not needed. |
| Fantastic Fan | Open, fan OFF or AUTO | As needed | Close vent in extreme winds (towing) |
|  |  |  |  |
|  |  |  |  |